The firmware is cross-compiled, but the build system ends up using
'objcopy' instead of 'xtensa-elf-objcopy' by default.  Force it to
use the right one.

--- source/target_firmware/configure	2014-10-28 20:57:26.834436561 +0100
+++ source/target_firmware/configure	2014-10-28 20:57:29.666436530 +0100
@@ -11,6 +11,7 @@ mkdir -p build
 cat > "$TOOLCHAIN_FILE" <<EOF
 INCLUDE(CMakeForceCompiler)
 
+SET(CMAKE_OBJCOPY xtensa-elf-objcopy)
 SET(CMAKE_SYSTEM_PROCESSOR xtensa)
 SET(CMAKE_FIND_ROOT_PATH ${TOOLCHAIN}/$TARGET)
 SET(CMAKE_STRIP :)
