From eb7a20a3616085d46aa6b4b4224e15587ec67e6e Mon Sep 17 00:00:00 2001
From: Li Qiang <liqiang6-s@360.cn>
Date: Mon, 28 Nov 2016 17:49:04 -0800
Subject: [PATCH] watchdog: 6300esb: add exit function

When the Intel 6300ESB watchdog is hot unplug. The timer allocated
in realize isn't freed thus leaking memory leak. This patch avoid
this through adding the exit function.

http://git.qemu.org/?p=qemu.git;a=patch;h=eb7a20a3616085d46aa6b4b4224e15587ec67e6e
this patch is from qemu-git.

Signed-off-by: Li Qiang <liqiang6-s@360.cn>
Message-Id: <583cde9c.3223ed0a.7f0c2.886e@mx.google.com>
Signed-off-by: Paolo Bonzini <pbonzini@redhat.com>
---
 hw/watchdog/wdt_i6300esb.c |    9 +++++++++
 1 files changed, 9 insertions(+), 0 deletions(-)

diff --git a/hw/watchdog/wdt_i6300esb.c b/hw/watchdog/wdt_i6300esb.c
index a83d951..49b3cd1 100644
--- a/hw/watchdog/wdt_i6300esb.c
+++ b/hw/watchdog/wdt_i6300esb.c
@@ -428,6 +428,14 @@ static void i6300esb_realize(PCIDevice *dev, Error **errp)
     /* qemu_register_coalesced_mmio (addr, 0x10); ? */
 }
 
+static void i6300esb_exit(PCIDevice *dev)
+{
+    I6300State *d = WATCHDOG_I6300ESB_DEVICE(dev);
+
+    timer_del(d->timer);
+    timer_free(d->timer);
+}
+
 static WatchdogTimerModel model = {
     .wdt_name = "i6300esb",
     .wdt_description = "Intel 6300ESB",
@@ -441,6 +449,7 @@ static void i6300esb_class_init(ObjectClass *klass, void *data)
     k->config_read = i6300esb_config_read;
     k->config_write = i6300esb_config_write;
     k->realize = i6300esb_realize;
+    k->exit = i6300esb_exit;
     k->vendor_id = PCI_VENDOR_ID_INTEL;
     k->device_id = PCI_DEVICE_ID_INTEL_ESB_9;
     k->class_id = PCI_CLASS_SYSTEM_OTHER;
-- 
1.7.0.4

