Don't install a zeroed encryption key:

https://w1.fi/security/2017-1/wpa-packet-number-reuse-with-replayed-messages.txt

Patch copied from upstream:
https://w1.fi/security/2017-1/rebased-v2.6-0004-Prevent-installation-of-an-all-zero-TK.patch

From 8f82bc94e8697a9d47fa8774dfdaaede1084912c Mon Sep 17 00:00:00 2001
From: Mathy Vanhoef <Mathy.Vanhoef@cs.kuleuven.be>
Date: Fri, 29 Sep 2017 04:22:51 +0200
Subject: [PATCH 4/8] Prevent installation of an all-zero TK

Properly track whether a PTK has already been installed to the driver
and the TK part cleared from memory. This prevents an attacker from
trying to trick the client into installing an all-zero TK.

This fixes the earlier fix in commit
ad00d64e7d8827b3cebd665a0ceb08adabf15e1e ('Fix TK configuration to the
driver in EAPOL-Key 3/4 retry case') which did not take into account
possibility of an extra message 1/4 showing up between retries of
message 3/4.

Signed-off-by: Mathy Vanhoef <Mathy.Vanhoef@cs.kuleuven.be>
---
 src/common/wpa_common.h | 1 +
 src/rsn_supp/wpa.c      | 5 ++---
 src/rsn_supp/wpa_i.h    | 1 -
 3 files changed, 3 insertions(+), 4 deletions(-)

diff --git a/src/common/wpa_common.h b/src/common/wpa_common.h
index d200285..1021ccb 100644
--- a/src/common/wpa_common.h
+++ b/src/common/wpa_common.h
@@ -215,6 +215,7 @@ struct wpa_ptk {
 	size_t kck_len;
 	size_t kek_len;
 	size_t tk_len;
+	int installed; /* 1 if key has already been installed to driver */
 };
 
 struct wpa_gtk {
diff --git a/src/rsn_supp/wpa.c b/src/rsn_supp/wpa.c
index 7a2c68d..0550a41 100644
--- a/src/rsn_supp/wpa.c
+++ b/src/rsn_supp/wpa.c
@@ -510,7 +510,6 @@ static void wpa_supplicant_process_1_of_4(struct wpa_sm *sm,
 		os_memset(buf, 0, sizeof(buf));
 	}
 	sm->tptk_set = 1;
-	sm->tk_to_set = 1;
 
 	kde = sm->assoc_wpa_ie;
 	kde_len = sm->assoc_wpa_ie_len;
@@ -615,7 +614,7 @@ static int wpa_supplicant_install_ptk(struct wpa_sm *sm,
 	enum wpa_alg alg;
 	const u8 *key_rsc;
 
-	if (!sm->tk_to_set) {
+	if (sm->ptk.installed) {
 		wpa_dbg(sm->ctx->msg_ctx, MSG_DEBUG,
 			"WPA: Do not re-install same PTK to the driver");
 		return 0;
@@ -659,7 +658,7 @@ static int wpa_supplicant_install_ptk(struct wpa_sm *sm,
 
 	/* TK is not needed anymore in supplicant */
 	os_memset(sm->ptk.tk, 0, WPA_TK_MAX_LEN);
-	sm->tk_to_set = 0;
+	sm->ptk.installed = 1;
 
 	if (sm->wpa_ptk_rekey) {
 		eloop_cancel_timeout(wpa_sm_rekey_ptk, sm, NULL);
diff --git a/src/rsn_supp/wpa_i.h b/src/rsn_supp/wpa_i.h
index 9a54631..41f371f 100644
--- a/src/rsn_supp/wpa_i.h
+++ b/src/rsn_supp/wpa_i.h
@@ -24,7 +24,6 @@ struct wpa_sm {
 	struct wpa_ptk ptk, tptk;
 	int ptk_set, tptk_set;
 	unsigned int msg_3_of_4_ok:1;
-	unsigned int tk_to_set:1;
 	u8 snonce[WPA_NONCE_LEN];
 	u8 anonce[WPA_NONCE_LEN]; /* ANonce from the last 1/4 msg */
 	int renew_snonce;
-- 
2.7.4

